**PEL Turbo DC Air Conditioner 2 Ton**

|  |  |  |
| --- | --- | --- |
| **SPECIFICATION** | **24K Turbo DC** | |
| **Rated Capacity - Cooling** | **7034(2000-8000) W** | |
| **Rated Running Current - Cooling** | **8.7(1.7-15.5) A** | |
| **Maximum Current** | **15.5 A** | |
| **Rated Power Cooling** | **1950(350-3200) W** | |
| **Maximum Power** | **3200 W** | |
| **Seasonal / Energy Efficiency Ratio (SEER/EER)** | **4.30 W/W** | |
| **Power supply source** | **220~240V/50Hz V/Ph/Hz** | |
| **Refrigerant** | **R410a** | |
| **Air Flow Volume** | **1150 m3/h** | |
| **Outdoor Noise level** | **45/59 dB(A)** | |
| **Indoor unit weight （Net )** | **15 Kg** | |
| **Outdoor unit weight (Net )** | **59 Kg** | |
| **Net Dimension - Indoor (WidthxDepthxHeight)** | **1095x327x235 mm** | |
| **Net Dimension - Outdoor (WidthxDepthxHeight)** | **953×808×433 mm** | |
| Compressor Warranty | 10 Years |
| PCB Kit Warranty | 02 Years |
| Parts Warranty | 1 Year |

**Split AC installation Cost:**

|  |  |
| --- | --- |
| **Description (Wall Mounted Split AC 1-2 Ton)** | **Tariff (PKR)** |
| **PEL Technician Installation** | **3000** |
| **Dismantling Charges in case of previous AC** | **1300** |
| **Extra Copper Pipe (RFT)** | **350** |
| **PVC Drain Pipe (RFT)** | **60** |
| **Simple Grooving without Pipe Concealing (RFT)** | **50** |
| **Iron Frame Charges (Powder Coated)** | **950** |
| **Filling of Holes with white Plaster of Paris (RFT)** | **200** |
| **PVC Duct for Refrigeration pipe (RFT)** | **240** |
| **Additional Gas Charging (if required) \*\*In case of more than 10ft outdoor height** | **(R-22) 200 Per RFT (R410a) 450 Per RFT** |